|  |  |  |
| --- | --- | --- |
| **Cairo University** | **CMP201** | **Total: 20 Points** |
| **Faculty of Engineering** | **Microprocessor Systems** | **2017-2018** |
| **Computer Eng. Department** | **Midterm Exam** | **One Hour** |

**This is an open-book, open notes exam. All electronic devices - Except calculators - are forbidden.
Make any reasonable assumptions (if necessary)**

1. **[10] Identify the choice that best completes the statement or answers the question**

|  |  |
| --- | --- |
|  **Answer** | **1- In the Intel architecture, there are actually several buses connecting the CPU to the rest of the computer. Which of the following is not such a bus?** |
|  | a) The control bus | b) The logic bus | c) The data bus | d) The address bus |
|   | **2- In the Intel architecture, the “program counter”, which determines where the next instruction is located, is in fact realized by means of which pair of registers?** |
| a) SP and CS | b) IP and CS | c) IP and DS | d) SP and DS |
|   | **3- Find the memory address of the next instruction executed by the microprocessor for the following CS:IP combination CS = 2000H and IP = 1000H** |
| a) 20010 | b) 21000 | c) 2100 | d) 3000 |
|   | **4- Which flag(s) let you check for signed overflow?** |
| a) Overflow | b) Direction | c) Interrupt | d) Carry |
|   | **5- If DS = 90A3H, then the range of physical addresses for the data segment is:** |
| a) 90A30H – 9FA30H | b) 090A3 – 190A2H | c) 00000H – 090A3H | d) 90A30 – A0A2FH |
|   | **6- A segment hex value of 35AB together with an offset hex value of 7E21 corresponds to what physical (hex) address?** |
| a)817BB  | B)3D6D1  | c) 3D8D1 | d)827BB |
|   | **7- one of the following is a legal 8086 instruction?** |
| 1. dec ip
 | 1. inc ax,1
 | 1. inc [si]
 | 1. add bx, [si]
 |
|   | **8- Which of the following variables uses the most amount of RAM?** |
| a) X DB 300 dup(‘A’)  | b) Z DD 40 dup (0) | c) Y DQ 255  | d) W DW 200 dup (0) |
|   | **9- The BP register is typically used for accessing** |
| 1. data segment
 | 1. stack
 | 1. strings
 | 1. memory
 |
|   | **10- To reserve 64-bits in memory --------directive is used.** |
| 1. DT
 | 1. DQ
 | 1. DW
 | 1. DD
 |
|   | **11- Which of the following will generate assembly errors?** |
| a) var1 db 1101b, 22, 35 | b) var3 db '$','98778', | c) var2 db "ABCDE", 18 | d)None of the above |
|   | **12-Assume that the AX register contains the value 6521 H. What will be the contents of AX after execution the instruction:SUB AL, AH** |
| 1. 65BC H
 | 1. 4421 H
 | 1. BC21 H
 | 1. 6544 H
 |
|   | **13- The instruction PUSH AL** |
| a) Decrement SP by 2 and push a word to stack | b) Increment SP by 2 and push a word to stack | c) Decrement SP by 1 and push a AL to stack | d) None of the above  |
|   | **14- What will be the value of the Overflow flag after executing the following instructions?mov al, 80hadd al,92h**  |
| 1. OF = 0
 | 1. OF = 1
 | 1. OF = Not affected
 | 1. OF = Unknown
 |
|   | **15- The value of AX after executing the following code is --------MOV AX, 1461hMOV DS, AXMOV AL, 05MOV AH, 07** |
| 1. 1461h
 | 1. 0705h
 | 1. 0507h
 | 1. 6114h
 |
|   | **16- In the following data definition, assume that List2 begins at offset 2000h. What is the offset of the third value (5)?List2 dw 3,4,5,6,7** |
| a) 2004h  | b) 2006  | c) 2002 | d) 2003 |
|   | **17- What will be the contents of register AL after the following has been executedMOV BX, F78CMOV AL, 7EADD AL, BL** |
| a) 6A and carry flag is set  | 0A and carry flag is set | 6A and carry flag is reset  | 0A and carry flag is reset |
|   | **18-Which of the following is an invalid instruction?** |
| 1. add dx,dx
 | 1. MOV AX, CS
 | 1. sub bar,5
 | 1. MOV AL, DI
 |
|   | **19-The conditional branch instruction JNS performs the operations when if**  |
| 1. SF=0
 | 1. ZF =0
 | 1. CF=0
 | 1. SF=1
 |
|   | **20-What values of AX and BX will cause the following jump to occur:CMP BX, AXJG THERE** |
| 1. AX=2345H, BX=1234H
 | 1. AX = BX
 | 1. AX=C000H, BX=0002H
 | 1. AX=0002H, BX=C000H
 |

1. **[4] Identify whether the following instructions are Valid or Invalid. Explain the reason for each Invalid instruction.**

|  |  |  |
| --- | --- | --- |
| **Instruction**  | **V/I** | **Reason** |
| MOV BP, SP  |  |  |
| add ax, [dx+ Yword]  |  |  |
| mov cx, [bx+4]  |  |  |
| MOV ES, N |  |  |
| MOV DX, DX |  |  |
| MOV M, N |  |  |
| MOV AX, SI+DI+2 |  |  |
| MOV BX, AX+1 |  |  |

**3- [2] Using one line only**

a) Declare three 4-byte variables of memory starting at; address “Z”, and initialized to 1, 2, and 3, respectively.

b) Array of **10 double words** initialized to **1, 2, ..., 10**.

c) A string with a message “**Press any key to continue**” ready for output using int 21h / AH=9

**d)** Declare 4-bytes array **of 100** numbers, all initialized to 0, starting at memory location “**Marks**”.

**4- [4] Write a complete assembly program that draws a 20\*20 pixels square moving from left to right. In your code, make a macro that draws a square at certain point with a specific colour.**